min_slic3r_version = 2.3.0-alpha2
0.0.7 Updated start g-code for Creality printers
0.0.6 Added filament profiles, adjusted temperatures, updated start g-code for some models.
0.0.5 Added 0.08mm SUPERDETAIL and 0.28mm SUPERDRAFT print profiles. Updated OPTIMAL print profile.
0.0.4 Added initial CR-10 profile, end g-code improvements.
min_slic3r_version = 2.3.0-alpha0
0.0.3 Added Ender-2, Ender-3 BLTouch, updated Ender-3 bed texture.
min_slic3r_version = 2.2.0-alpha3
0.0.2 Updated for PrusaSlicer 2.2.0-rc
0.0.2-beta Update for PrusaSlicer 2.2.0-beta
0.0.2-alpha1 Extended list of default filaments to be installed
0.0.2-alpha0 Print bed textures are now configurable from the Preset Bundle. Requires PrusaSlicer 2.2.0-alpha3 and newer.
# The following line (max_slic3r_version) forces the users of PrusaSlicer 2.2.0-alpha3 and newer to update the profiles to 1.1.1-alpha3 and newer,
# so they will see the print bed.
max_slic3r_version = 2.2.0-alpha2
min_slic3r_version = 2.2.0-alpha0
0.0.1 Initial version
